#####################################################################################################################
Database created by the Theoretical and Applied Aerodynamic Research Group @ University of Naples Federico II

Jet flows emanating from parametric nozzle geometries.
3 geometrical parameters: fa*; ARout; nout.

Multi-Fidelity database of flow fields: Low-Fidelity (RANS) obtained with SU2 software; High-Fidelity (LES) obtained with CharLes software

Please, refer to "Multi-fidelity Autoencoders: RANS-LES jet flow predictions" published on ......

	- database_RANS_LF.npy:		numpy array containing the RANS (Low-Fidelity) database
	- parameters_RANS_LF.npy:	numpy array containing the design parameters of the RANS simulations
	- database_LES_HF.npy:		numpy array containing the LES (High-Fidelity) database
	- parameters_LES_HF.npy:	numpy array containing the design parameters of the LES simulations

Dimension of database numpy arrays:
[num_cases, channels, number of I pixels, number of J pixels]

	- database_RANS_LF.npy: (92, 12, 128, 128)
	- database_LES_HF.npy:	(18, 12, 128, 128)

Channels description:
	- 0:	x grid coordinates in the x-z plane of the symmetry section (y=0)
	- 1:	z grid coordinates in the x-z plane of the symmetry section (y=0)
	- 2:	u velocity component in the x-z plane of the symmetry section (y=0)
	- 3:	v velocity component in the x-z plane of the symmetry section (y=0)

	- 4:	y grid coordinates in the y-z plane of the section at x=1m
	- 5:	z grid coordinates in the y-z plane of the section at x=1m
	- 6:	u velocity component in the y-z plane of the section at x=1m
	- 7:	v velocity component in the y-z plane of the section at x=1m

	- 8:	y grid coordinates in the y-z plane of the section at x=2m
	- 9:	z grid coordinates in the y-z plane of the section at x=2m
	- 10:	u velocity component in the y-z plane of the section at x=2m
	- 11:	v velocity component in the y-z plane of the section at x=2m




